(module 08055F104K4T2A (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value CAP_0805_AVX (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.054in/1.37mm" (at 4.103 0) (layer Cmts.User))
  (fp_text user "0.111in/2.821mm" (at 0 -3.733) (layer Cmts.User))
  (fp_text user "0.052in/1.31mm" (at 0 3.733) (layer Cmts.User))
  (pad 1 smd rect (at -1.0328 0) (size 0.7556 1.37) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 1.0328 0) (size 0.7556 1.37) (layers F.Cu F.Paste F.Mask))
)
