(module 1B22AN (layer F.Cu)
  (fp_text reference REF** (at 10.16 22.86) (layer F.SilkS))
  (fp_text value 1B22_N_12_ADI (at 10.16 22.86) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.1in/2.54mm" (at -3.048 1.27) (layer Cmts.User))
  (fp_text user "0.06in/1.524mm" (at 23.368 0) (layer Cmts.User))
  (fp_text user "0.8in/20.32mm" (at 10.16 -6.223) (layer Cmts.User))
  (fp_text user "0.06in/1.524mm" (at 0 51.943) (layer Cmts.User))
  (fp_text user "*" (at -2.286 0) (layer F.Fab))
  (fp_text user "*" (at 0 -1.524) (layer F.SilkS))
  (pad 1 thru_hole rect (at 0 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 16 thru_hole circle (at 0 38.1) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 17 thru_hole circle (at 0 40.64) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 18 thru_hole circle (at 0 43.18) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 19 thru_hole circle (at 0 45.72) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 20 thru_hole circle (at 20.32 45.72) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 21 thru_hole circle (at 20.32 43.18) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 22 thru_hole circle (at 20.32 40.64) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 23 thru_hole circle (at 20.32 38.1) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 24 thru_hole circle (at 20.32 35.56) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 25 thru_hole circle (at 20.32 33.02) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
  (pad 38 thru_hole circle (at 20.32 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask))
)
