(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "VL53L4CDV0DH_1" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 25.4 10.16 0))
    (property "Value" "VL53L4CDV0DH/1" (id 1) (at 25.4 7.62 0))
    (property "Footprint" "LGA12_STM" (id 2) (at 0 0 0))
    (property "Datasheet" "VL53L4CDV0DH/1" (id 3) (at 0 0 0))
    (property "ki_keywords" "VL53L4CDV0DH/1" (id 4) (at 0 0 0))
    (property "ki_locked" "" (id 5) (at 0 0 0))
    (property "ki_fp_filters" "LGA12_STM" (id 6) (at 0 0 0))
    (symbol "VL53L4CDV0DH_1_0_1"
      (pin power_in line (at 0 0 0) (length 7.62)
        (name "AVDDVCSEL")
        (number "1")
      )
      (pin power_out line (at 0 -2.54 0) (length 7.62)
        (name "AVSSVCSEL")
        (number "2")
      )
      (pin power_out line (at 0 -5.08 0) (length 7.62)
        (name "GND")
        (number "3")
      )
      (pin power_out line (at 0 -7.62 0) (length 7.62)
        (name "GN2")
        (number "4")
      )
      (pin unspecified line (at 0 -10.16 0) (length 7.62)
        (name "XSHUT")
        (number "5")
      )
      (pin power_out line (at 0 -12.7 0) (length 7.62)
        (name "GND3")
        (number "6")
      )
      (pin bidirectional line (at 50.8 -12.7 180) (length 7.62)
        (name "GPIO1")
        (number "7")
      )
      (pin no_connect line (at 50.8 -10.16 180) (length 7.62)
        (name "DNC")
        (number "8")
      )
      (pin bidirectional line (at 50.8 -7.62 180) (length 7.62)
        (name "SDA")
        (number "9")
      )
      (pin bidirectional line (at 50.8 -5.08 180) (length 7.62)
        (name "SCL")
        (number "10")
      )
      (pin power_in line (at 50.8 -2.54 180) (length 7.62)
        (name "AVDD")
        (number "11")
      )
      (pin power_out line (at 50.8 0 180) (length 7.62)
        (name "GND4")
        (number "12")
      )
    )
  )
)
