(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "MT25QL128ABA1ESE-0SIT" (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 27.94 10.16 0))
    (property "Value" "MT25QL128ABA1ESE-0SIT" (id 1) (at 27.94 7.62 0))
    (property "Footprint" "SOP2_8PIN_208MIL_MRN" (id 2) (at 0 0 0))
    (property "Datasheet" "MT25QL128ABA1ESE-0SIT" (id 3) (at 0 0 0))
    (property "ki_keywords" "MT25QL128ABA1ESE-0SIT" (id 4) (at 0 0 0))
    (property "ki_locked" "" (id 5) (at 0 0 0))
    (property "ki_fp_filters" "SOP2_8PIN_208MIL_MRN SOP2_8PIN_208MIL_MRN-M SOP2_8PIN_208MIL_MRN-L" (id 6) (at 0 0 0))
    (symbol "MT25QL128ABA1ESE-0SIT_0_1"
      (pin input line (at 0 0 0) (length 7.62)
        (name "S#")
        (number "1")
      )
      (pin bidirectional line (at 0 -2.54 0) (length 7.62)
        (name "DQ1")
        (number "2")
      )
      (pin bidirectional line (at 0 -5.08 0) (length 7.62)
        (name "W#/DQ2")
        (number "3")
      )
      (pin power_out line (at 0 -7.62 0) (length 7.62)
        (name "VSS")
        (number "4")
      )
      (pin bidirectional line (at 55.88 -7.62 180) (length 7.62)
        (name "DQ0")
        (number "5")
      )
      (pin input line (at 55.88 -5.08 180) (length 7.62)
        (name "C")
        (number "6")
      )
      (pin bidirectional line (at 55.88 -2.54 180) (length 7.62)
        (name "DQ3/HOLD#")
        (number "7")
      )
      (pin power_in line (at 55.88 0 180) (length 7.62)
        (name "VCC")
        (number "8")
      )
    )
  )
)
