(module 2SC5200-OQ (layer F.Cu)
  (fp_text reference REF** (at 5.450001 0.496) (layer F.SilkS))
  (fp_text value TO-3PL_TOS (at 5.450001 0.496) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.069in/1.753mm" (at 0 -3.8855) (layer Cmts.User))
  (fp_text user "0.069in/1.753mm" (at 10.900001 4.8775) (layer Cmts.User))
  (fp_text user "TAB" (at 5.450001 -2.1075) (layer F.Fab))
  (pad 1 thru_hole circle (at 0 0) (size 1.7526 1.7526) (drill 1.2446) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 5.450001 0) (size 1.7526 1.7526) (drill 1.2446) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 10.900001 0) (size 1.7526 1.7526) (drill 1.2446) (layers *.Cu *.Mask))
)
