(module 355015KJT (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value RES_3550_TEC (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.207in/5.258mm" (at 8.6995 0) (layer Cmts.User))
  (fp_text user "0.461in/11.709mm" (at 0 -5.6769) (layer Cmts.User))
  (fp_text user "0.241in/6.121mm" (at 0 5.6769) (layer Cmts.User))
  (pad 1 smd rect (at -4.4577 0) (size 2.794 5.2578) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 4.4577 0) (size 2.794 5.2578) (layers F.Cu F.Paste F.Mask))
)
