(module Package_SON:WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm (layer F.Cu) (tedit 61B6F17F)
  (descr "WSON, 6 Pin (http://www.ti.com/lit/ds/symlink/tps61040.pdf#page=35), generated with kicad-footprint-generator ipc_noLead_generator.py")
  (tags "WSON NoLead")
  (attr smd)
  (fp_text reference REF** (at 0 -1.95) (layer F.SilkS))
  (fp_text value WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm (at 0 1.95) (layer F.Fab))
  (fp_text user %R (at 0 0) (layer F.Fab))
  (pad "" smd roundrect (at 0 0.4) (size 0.81 0.64) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at 0 -0.4) (size 0.81 0.64) (layers F.Paste) (roundrect_rratio 0.25))
  (pad 7 smd rect (at 0 0) (size 1 1.6) (layers F.Cu F.Mask))
  (pad 6 smd rect (at 0.8875 -0.65) (size 0.375 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 0.8875 0) (size 0.375 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 0.8875 0.65) (size 0.375 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -0.8875 0.65) (size 0.375 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -0.8875 0) (size 0.375 0.4) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -0.8875 -0.65) (size 0.375 0.4) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Package_SON.3dshapes/WSON-6-1EP_2x2mm_P0.65mm_EP1x1.6mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
