(module Package_SO:SOIC-8_3.9x4.9mm_P1.27mm (layer F.Cu) (tedit 61A79C1F)
  (descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
  (tags "SOIC SO")
  (attr smd)
  (fp_text reference REF** (at 0 -3.4) (layer F.SilkS))
  (fp_text value SOIC-8_3.9x4.9mm_P1.27mm (at 0 3.4) (layer F.Fab))
  (fp_text user %R (at 0 0) (layer F.Fab))
  (pad 8 smd rect (at 2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -2.475 1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -2.475 0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -2.475 -0.635) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -2.475 -1.905) (size 1.95 0.6) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
