(footprint "AAA-Contact" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at -2.58 -5.1 unlocked) (layer "F.SilkS"))
  (fp_text value "AAA-Contact" (at -0.63 -1.52 unlocked) (layer "F.Fab"))
  (fp_text user "${REFERENCE}" (at -1.15 0.14 unlocked) (layer "F.Fab"))
  (pad "1" thru_hole oval (at -1.52 -3.61) (size 5 2) (drill oval 3.35 0.75) (layers "*.Cu" "*.Mask"))
  (model "C:/Users/davidh/Documents/----Downloaded Electronics Libraries/Battery/Clip/5204/3D/5204.stp"
    (offset (xyz -2.9 2.9 3))
    (scale (xyz 1 1 1))
    (rotate (xyz -90 0 0))
  )
)
