(module ABLS-16.000MHZ-B2-T (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value XTAL_ABLS-16_ABR (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0in/0mm" (at -7.7978 0) (layer Cmts.User))
  (fp_text user "0.03in/0.762mm" (at 7.7978 0) (layer Cmts.User))
  (fp_text user "0.374in/9.5mm" (at 0 -4.9022) (layer Cmts.User))
  (fp_text user "0.174in/4.42mm" (at -4.7498 4.2672) (layer Cmts.User))
  (pad 1 smd rect (at -4.7498 0) (size 4.4196 0.762) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 4.7498 0) (size 4.4196 0.762) (layers F.Cu F.Paste F.Mask))
)
