(module ADG732BCPZ (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value CP_48_1_ADI (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.02in/0.5mm" (at -5.4356 -2.5) (layer Cmts.User))
  (fp_text user "0.032in/0.813mm" (at -3.4036 -6.4516) (layer Cmts.User))
  (fp_text user "0.01in/0.254mm" (at -6.4516 3.4036) (layer Cmts.User))
  (fp_text user "0.268in/6.807mm" (at 0 8.9916) (layer Cmts.User))
  (fp_text user "0.268in/6.807mm" (at 8.9916 0.635) (layer Cmts.User))
  (fp_text user "0.207in/5.258mm" (at 0 5.6769) (layer Cmts.User))
  (fp_text user "0.207in/5.258mm" (at 5.6769 -0.635) (layer Cmts.User))
  (fp_text user "*" (at -4.445 -3) (layer F.SilkS))
  (fp_text user "*" (at -2.9972 -3) (layer F.Fab))
  (pad 1 smd rect (at -3.4036 -2.75 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -3.4036 -2.250001 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -3.4036 -1.749999 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -3.4036 -1.25 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -3.4036 -0.750001 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -3.4036 -0.25 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -3.4036 0.25 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -3.4036 0.750001 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at -3.4036 1.25 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at -3.4036 1.749999 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at -3.4036 2.250001 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at -3.4036 2.75 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at -2.75 3.4036) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at -2.250001 3.4036) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at -1.749999 3.4036) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at -1.25 3.4036) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd rect (at -0.750001 3.4036) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd rect (at -0.25 3.4036) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd rect (at 0.25 3.4036) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd rect (at 0.750001 3.4036) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 21 smd rect (at 1.25 3.4036) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 22 smd rect (at 1.749999 3.4036) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 23 smd rect (at 2.250001 3.4036) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 24 smd rect (at 2.75 3.4036) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 25 smd rect (at 3.4036 2.75 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 26 smd rect (at 3.4036 2.250001 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 27 smd rect (at 3.4036 1.749999 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 28 smd rect (at 3.4036 1.25 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 29 smd rect (at 3.4036 0.750001 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 30 smd rect (at 3.4036 0.25 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 31 smd rect (at 3.4036 -0.25 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 32 smd rect (at 3.4036 -0.750001 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 33 smd rect (at 3.4036 -1.25 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 34 smd rect (at 3.4036 -1.749999 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 35 smd rect (at 3.4036 -2.250001 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 36 smd rect (at 3.4036 -2.75 90) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 37 smd rect (at 2.75 -3.4036) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 38 smd rect (at 2.250001 -3.4036) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 39 smd rect (at 1.749999 -3.4036) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 40 smd rect (at 1.25 -3.4036) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 41 smd rect (at 0.750001 -3.4036) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 42 smd rect (at 0.25 -3.4036) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 43 smd rect (at -0.25 -3.4036) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 44 smd rect (at -0.750001 -3.4036) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 45 smd rect (at -1.25 -3.4036) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 46 smd rect (at -1.749999 -3.4036) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 47 smd rect (at -2.250001 -3.4036) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 48 smd rect (at -2.75 -3.4036) (size 0.254 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 49 smd rect (at 0 0) (size 5.2578 5.2578) (layers F.Cu F.Paste F.Mask))
)
