(module ADP1607ACPZN001-R7 (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value CP_6_3_ADI (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "Default Padstyle: RX25p78Y9p81D0T" (at 0 9.128) (layer Cmts.User))
  (fp_text user "Heat Tab Padstyle: RX39p37Y62p99D0T" (at 0 10.652) (layer Cmts.User))
  (fp_text user "Alt 1 Padstyle: OX60Y90D30P" (at 0 13.699999) (layer Cmts.User))
  (fp_text user "Alt 2 Padstyle: OX90Y60D30P" (at 0 15.223999) (layer Cmts.User))
  (fp_text user "0.079in/2mm" (at 0 -7.508) (layer Cmts.User))
  (fp_text user "0.014in/0.35mm" (at -0.825 -3.698) (layer Cmts.User))
  (fp_text user "0.026in/0.65mm" (at -4.0254 -0.325) (layer Cmts.User))
  (fp_text user "0.079in/2mm" (at 4.0254 0) (layer Cmts.User))
  (fp_text user "0.079in/2mm" (at 0 4.048) (layer Cmts.User))
  (fp_text user "LX" (at 0 -7.508) (layer Cmts.User))
  (fp_text user "FOOT_L" (at -0.825 -3.698) (layer Cmts.User))
  (fp_text user "RP" (at -4.0254 -0.325) (layer Cmts.User))
  (fp_text user "BODY_H" (at 4.0254 0) (layer Cmts.User))
  (fp_text user "BODY_W" (at 0 4.048) (layer Cmts.User))
  (fp_text user "0.026in/0.65mm" (at -4.0254 -0.325) (layer Cmts.User))
  (fp_text user "0.01in/0.249mm" (at 4.0254 -0.65) (layer Cmts.User))
  (fp_text user "0.077in/1.955mm" (at 0 -3.413) (layer Cmts.User))
  (fp_text user "0.026in/0.655mm" (at -0.9774 2.778) (layer Cmts.User))
  (fp_text user "0.063in/1.6mm" (at 3.413 0) (layer Cmts.User))
  (fp_text user "0.039in/1mm" (at 0 4.048) (layer Cmts.User))
  (fp_text user "12" (at 3.2004 -11.167999) (layer Cmts.User))
  (fp_text user "0" (at 4.51 -11.167999) (layer Cmts.User))
  (fp_text user "13.78" (at 4.16 -10.659999) (layer Cmts.User))
  (fp_text user "9.81" (at -3.048 -11.040999) (layer Cmts.User))
  (fp_text user "11.81" (at -3.048 -10.659999) (layer Cmts.User))
  (fp_text user "(2x Scale)" (at 0 -15.485999) (layer Cmts.User))
  (pad 1 smd rect (at -0.9774 -0.649999) (size 0.6548 0.2492) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -0.9774 0) (size 0.6548 0.2492) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -0.9774 0.649999) (size 0.6548 0.2492) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 0.9774 0.649999) (size 0.6548 0.2492) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 0.9774 0) (size 0.6548 0.2492) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 0.9774 -0.649999) (size 0.6548 0.2492) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 0 0) (size 1 1.6) (layers F.Cu F.Paste F.Mask))
)
