(footprint "AK4619VN_AKM" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tags "AK4619VN ")
  (attr smd)
  (fp_text reference "REF**" (at 0 0 unlocked) (layer F.SilkS))
  (fp_text value AK4619VN_AKM (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "*" (at -3.135 -2) (layer F.SilkS))
  (fp_text user "*" (at -2.0936 -2) (layer F.Fab))
  (fp_text user "*" (at -3.135 -2 unlocked) (layer "F.SilkS"))
  (fp_text user "*" (at -2.0936 -2 unlocked) (layer "F.Fab"))
  (pad "1" smd rect (at -2.2968 -1.749999 90) (size 0.254 0.4064) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at -2.2968 -1.25 90) (size 0.254 0.4064) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at -2.2968 -0.750001 90) (size 0.254 0.4064) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd rect (at -2.2968 -0.25 90) (size 0.254 0.4064) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "5" smd rect (at -2.2968 0.25 90) (size 0.254 0.4064) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "6" smd rect (at -2.2968 0.750001 90) (size 0.254 0.4064) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "7" smd rect (at -2.2968 1.25 90) (size 0.254 0.4064) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "8" smd rect (at -2.2968 1.749999 90) (size 0.254 0.4064) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "9" smd rect (at -1.749999 2.2968) (size 0.254 0.4064) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "10" smd rect (at -1.25 2.2968) (size 0.254 0.4064) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "11" smd rect (at -0.750001 2.2968) (size 0.254 0.4064) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "12" smd rect (at -0.25 2.2968) (size 0.254 0.4064) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "13" smd rect (at 0.25 2.2968) (size 0.254 0.4064) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "14" smd rect (at 0.750001 2.2968) (size 0.254 0.4064) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "15" smd rect (at 1.25 2.2968) (size 0.254 0.4064) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "16" smd rect (at 1.749999 2.2968) (size 0.254 0.4064) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "17" smd rect (at 2.2968 1.749999 90) (size 0.254 0.4064) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "18" smd rect (at 2.2968 1.25 90) (size 0.254 0.4064) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "19" smd rect (at 2.2968 0.750001 90) (size 0.254 0.4064) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "20" smd rect (at 2.2968 0.25 90) (size 0.254 0.4064) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "21" smd rect (at 2.2968 -0.25 90) (size 0.254 0.4064) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "22" smd rect (at 2.2968 -0.750001 90) (size 0.254 0.4064) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "23" smd rect (at 2.2968 -1.25 90) (size 0.254 0.4064) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "24" smd rect (at 2.2968 -1.749999 90) (size 0.254 0.4064) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "25" smd rect (at 1.749999 -2.2968) (size 0.254 0.4064) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "26" smd rect (at 1.25 -2.2968) (size 0.254 0.4064) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "27" smd rect (at 0.750001 -2.2968) (size 0.254 0.4064) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "28" smd rect (at 0.25 -2.2968) (size 0.254 0.4064) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "29" smd rect (at -0.25 -2.2968) (size 0.254 0.4064) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "30" smd rect (at -0.750001 -2.2968) (size 0.254 0.4064) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "31" smd rect (at -1.25 -2.2968) (size 0.254 0.4064) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "32" smd rect (at -1.749999 -2.2968) (size 0.254 0.4064) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "33" smd rect (at 0 0) (size 3.7084 3.7084) (layers "F.Cu" "F.Paste" "F.Mask"))
)
