(module AP3211KTR-G1 (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value SOT23-6_DIO (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.042in/1.06mm" (at -1.1 -4.5466) (layer Cmts.User))
  (fp_text user "0.037in/0.95mm" (at -4.148 -0.475) (layer Cmts.User))
  (fp_text user "0.087in/2.2mm" (at 0 3.998) (layer Cmts.User))
  (fp_text user "0.026in/0.65mm" (at 4.148 -0.95) (layer Cmts.User))
  (pad 1 smd rect (at -1.1 -0.950001) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd oval (at -1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd oval (at -1.1 0.950001) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd oval (at 1.1 0.950001) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd oval (at 1.1 0) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd oval (at 1.1 -0.950001) (size 1.06 0.65) (layers F.Cu F.Paste F.Mask))
)
