(footprint "AS6221-AWLT-S_AMS" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tags "AS6221-AWLT-S ")
  (attr smd)
  (fp_text reference "REF**" (at 0 0 unlocked) (layer F.SilkS))
  (fp_text value AS6221-AWLT-S_AMS (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "A" (at -1.397 -0.2 unlocked) (layer "F.SilkS"))
  (fp_text user "A" (at -1.397 -0.2 unlocked) (layer "F.Fab"))
  (fp_text user "A" (at -1.397 -0.2 unlocked) (layer "B.SilkS"))
  (fp_text user "B" (at -1.397 0.2 unlocked) (layer "F.SilkS"))
  (fp_text user "B" (at -1.397 0.2 unlocked) (layer "F.Fab"))
  (fp_text user "B" (at -1.397 0.2 unlocked) (layer "B.SilkS"))
  (fp_text user "1" (at -0.4 -1.1557 90 unlocked) (layer "F.SilkS"))
  (fp_text user "1" (at -0.4 -1.1557 90 unlocked) (layer "F.Fab"))
  (fp_text user "1" (at -0.4 -1.1557 90 unlocked) (layer "B.SilkS"))
  (fp_text user "3" (at 0.4 -1.1557 90 unlocked) (layer "F.SilkS"))
  (fp_text user "3" (at 0.4 -1.1557 90 unlocked) (layer "F.Fab"))
  (fp_text user "3" (at 0.4 -1.1557 90 unlocked) (layer "B.SilkS"))
  (pad "A1" smd circle (at -0.4 -0.2) (size 0.2032 0.2032) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "A2" smd circle (at 0 -0.2) (size 0.2032 0.2032) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "A3" smd circle (at 0.4 -0.2) (size 0.2032 0.2032) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "B1" smd circle (at -0.4 0.2) (size 0.2032 0.2032) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "B2" smd circle (at 0 0.2) (size 0.2032 0.2032) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "B3" smd circle (at 0.4 0.2) (size 0.2032 0.2032) (layers "F.Cu" "F.Paste" "F.Mask"))
)
