(module AT27C256R-45PU (layer F.Cu)
  (fp_text reference REF** (at 7.9375 16.51) (layer F.SilkS))
  (fp_text value 28P6_ATM (at 7.9375 16.51) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.1in/2.54mm" (at -3.048 1.27) (layer Cmts.User))
  (fp_text user "0.052in/1.321mm" (at 18.923 0) (layer Cmts.User))
  (fp_text user "0.625in/15.875mm" (at 7.9375 -4.572) (layer Cmts.User))
  (fp_text user "0.052in/1.321mm" (at 0 37.592) (layer Cmts.User))
  (fp_text user "*" (at 1.2065 0) (layer F.Fab))
  (fp_text user "*" (at 0 -1.4224) (layer F.SilkS))
  (pad 1 thru_hole rect (at 0 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 0 2.54) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 0 5.08) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 0 7.62) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 0 10.16) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 0 12.7) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at 0 15.24) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at 0 17.78) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
  (pad 9 thru_hole circle (at 0 20.32) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
  (pad 10 thru_hole circle (at 0 22.86) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
  (pad 11 thru_hole circle (at 0 25.4) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
  (pad 12 thru_hole circle (at 0 27.94) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
  (pad 13 thru_hole circle (at 0 30.48) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
  (pad 14 thru_hole circle (at 0 33.02) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
  (pad 15 thru_hole circle (at 15.875 33.02) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
  (pad 16 thru_hole circle (at 15.875 30.48) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
  (pad 17 thru_hole circle (at 15.875 27.94) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
  (pad 18 thru_hole circle (at 15.875 25.4) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
  (pad 19 thru_hole circle (at 15.875 22.86) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
  (pad 20 thru_hole circle (at 15.875 20.32) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
  (pad 21 thru_hole circle (at 15.875 17.78) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
  (pad 22 thru_hole circle (at 15.875 15.24) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
  (pad 23 thru_hole circle (at 15.875 12.7) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
  (pad 24 thru_hole circle (at 15.875 10.16) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
  (pad 25 thru_hole circle (at 15.875 7.62) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
  (pad 26 thru_hole circle (at 15.875 5.08) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
  (pad 27 thru_hole circle (at 15.875 2.54) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
  (pad 28 thru_hole circle (at 15.875 0) (size 1.3208 1.3208) (drill 0.8128) (layers *.Cu *.Mask))
)
