(module Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.3x5.3mm (layer F.Cu) (tedit 638F6A67)
  (descr "QFN, 48 Pin (https://www.trinamic.com/fileadmin/assets/Products/ICs_Documents/TMC2041_datasheet.pdf#page=62), generated with kicad-footprint-generator ipc_noLead_generator.py")
  (tags "QFN NoLead")
  (attr smd)
  (fp_text reference "F.SilkS Designator" (at -0.635 -17.145) (layer F.SilkS))
  (fp_text value "F.Fab Properties" (at -0.635 17.78) (layer F.Fab))
  (fp_text user F.Adhes (at -0.635 -15.24) (layer F.Adhes))
  (fp_text user B.Adhes (at -0.635 -13.335) (layer B.Adhes))
  (fp_text user F.Paste (at -0.635 -11.43) (layer F.Paste))
  (fp_text user B.Paste (at -0.635 -9.525) (layer B.Paste))
  (fp_text user B.Fab (at -0.635 15.24) (layer B.Fab))
  (fp_text user F.Fab (at -0.635 13.335) (layer F.Fab))
  (fp_text user B.CrtYd (at -0.635 11.43) (layer B.CrtYd))
  (fp_text user F.CrtYd (at -0.635 9.525) (layer F.CrtYd))
  (fp_text user Margin (at -0.635 7.62) (layer Margin))
  (fp_text user Eco2.User (at -0.635 5.715) (layer Eco2.User))
  (fp_text user Eco1.User (at -0.635 3.81) (layer Eco1.User))
  (fp_text user Cmts.User (at -0.635 1.905) (layer Cmts.User))
  (fp_text user Dwgs.User (at -0.635 0) (layer Dwgs.User))
  (fp_text user B.Mask (at -0.635 -1.905) (layer B.Mask))
  (fp_text user F.Mask (at -0.635 -3.81) (layer F.Mask))
  (fp_text user B.SilkS (at -0.635 -5.715) (layer B.SilkS))
  (fp_text user F.SilkS (at -0.635 -7.62) (layer F.SilkS))
  (pad "Mask only" smd roundrect (at -13.97 11.43) (size 10 2) (layers F.Mask) (roundrect_rratio 0.25))
  (pad "no copper" smd roundrect (at -13.97 8.89) (size 10 2) (layers F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad "Paste only" smd roundrect (at -13.97 6.35) (size 10 2) (layers F.Paste) (roundrect_rratio 0.25))
  (pad Paste&Mask smd roundrect (at -13.97 3.81) (size 10 2) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad "with Mask" smd roundrect (at -13.97 1.27) (size 10 2) (layers F.Cu F.Mask) (roundrect_rratio 0.25))
  (pad "with Paste" smd roundrect (at -13.97 -1.27) (size 10 2) (layers F.Cu F.Paste) (roundrect_rratio 0.25))
  (pad "pure copper" smd roundrect (at -13.97 -3.81) (size 10 2) (layers F.Cu) (roundrect_rratio 0.25))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_P0.5mm_EP5.3x5.3mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
