(module Allegro_QFN-12-10-1EP_3x3mm_P0.5mm (layer F.Cu) (tedit 5AE4B66E)
  (descr "Allegro Microsystems 12-Lead (10-Lead Populated) Quad Flat Pack, 3x3mm Body, 0.5mm Pitch (http://www.allegromicro.com/~/media/Files/Datasheets/ACS711-Datasheet.ashx)")
  (tags "Allegro QFN 0.5")
  (attr smd)
  (fp_text reference REF** (at 0 -2.8) (layer F.SilkS))
  (pad 10 smd rect (at 0.23 -1.45) (size 0.3 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 0.73 -1.45) (size 0.3 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 0.23 1.45) (size 0.3 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 0.73 1.45) (size 0.3 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 1.43 0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 1.43 0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 1.43 -0.25) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 1.43 -0.75) (size 0.85 0.3) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -1.32 -0.5) (size 1.07 0.8) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.32 0.5) (size 1.07 0.8) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Sensor_Current.3dshapes/Allegro_QFN-12-10-1EP_3x3mm_P0.5mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
