(footprint "BATT_VL-2330/VCN_PAN" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tags "VL-2330/VCN ")
  (attr through_hole)
  (fp_text reference "REF**" (at 0 0 unlocked) (layer F.SilkS))
  (fp_text value BATT_VL-2330/VCN_PAN (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer F.Fab))
  (pad "1" thru_hole rect (at -5.085 -1.825) (size 2.667 2.667) (drill 2.159) (layers *.Cu *.Mask))
  (pad "2" thru_hole circle (at 5.085 1.825) (size 1.6002 1.6002) (drill 1.0922) (layers *.Cu *.Mask))
)
