(footprint "_09 Lib_PROJECTS_Infineon_Task Tracker Parts_Conversion_INP_2023_NPI Conversion_NPI Conversion_October-23_Working_BGA7P220_Altium_PQFN50P300X300X77-17N-V1.PcbLib_PQFN50P300X300X77-17N-V1" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (fp_text reference "Designator" (at -2.54 -2.032 unlocked) (layer "F.SilkS"))
  (fp_text value "Comment" (at 0 0 unlocked) (layer "F.Fab") hide)
  (fp_text user "${REFERENCE}" (at -3.643 0.385 unlocked) (layer "F.Fab"))
  (pad "1" smd rect (at -1.345 -0.75) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.025) (thermal_bridge_angle 45))
  (pad "2" smd rect (at -1.345 -0.25) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.025) (thermal_bridge_angle 45))
  (pad "3" smd rect (at -1.345 0.25) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.025) (thermal_bridge_angle 45))
  (pad "4" smd rect (at -1.345 0.75) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.025) (thermal_bridge_angle 45))
  (pad "5" smd rect (at -0.75 1.345 90) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.025) (thermal_bridge_angle 45))
  (pad "6" smd rect (at -0.25 1.345 90) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.025) (thermal_bridge_angle 45))
  (pad "7" smd rect (at 0.25 1.345 90) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.025) (thermal_bridge_angle 45))
  (pad "8" smd rect (at 0.75 1.345 90) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.025) (thermal_bridge_angle 45))
  (pad "9" smd rect (at 1.345 0.75) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.025) (thermal_bridge_angle 45))
  (pad "10" smd rect (at 1.345 0.25) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.025) (thermal_bridge_angle 45))
  (pad "11" smd rect (at 1.345 -0.25) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.025) (thermal_bridge_angle 45))
  (pad "12" smd rect (at 1.345 -0.75) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.025) (thermal_bridge_angle 45))
  (pad "13" smd rect (at 0.75 -1.345 90) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.025) (thermal_bridge_angle 45))
  (pad "14" smd rect (at 0.25 -1.345 90) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.025) (thermal_bridge_angle 45))
  (pad "15" smd rect (at -0.25 -1.345 90) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.025) (thermal_bridge_angle 45))
  (pad "16" smd rect (at -0.75 -1.345 90) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.025) (thermal_bridge_angle 45))
  (pad "17" smd rect (at 0 0) (size 1.7 1.7) (layers "F.Cu" "F.Paste" "F.Mask")
    (solder_paste_margin -0.85) (thermal_bridge_angle 45))
  (model "${KIPRJMOD}/ALTIUM_EMBEDDED_MODELS/PG-TSNP-16-12_Z8B00206082_V01_3D.stp"
    (offset (xyz 0 -0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz -0 -0 0))
  )
)
