(module BQ24170RGYR (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value RGY24_2P05X3P1 (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "1.968504E-02in/.5mm" (at -5.427 0) (layer Cmts.User))
  (fp_text user ".1362992in/3.462mm" (at 0 8.424001) (layer Cmts.User))
  (fp_text user ".2122835in/5.392mm" (at 9.719 0) (layer Cmts.User))
  (fp_text user ".03346in/.85mm" (at 2.696 -4.779) (layer Cmts.User))
  (fp_text user "1.102362E-02in/.28mm" (at -8.729 -2.25) (layer Cmts.User))
  (fp_text user "8.070866E-02in/2.05mm" (at 0 5.884001) (layer Cmts.User))
  (fp_text user ".1220472in/3.1mm" (at 5.909 0) (layer Cmts.User))
  (fp_text user "*" (at -0.75 -3.908342) (layer F.SilkS))
  (fp_text user "*" (at -0.75 -3.908342) (layer F.Fab))
  (pad 1 smd rect (at -0.750001 -2.695999) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.731 -2.250001 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.731 -1.749999 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -1.731 -1.25 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -1.731 -0.750001 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -1.731 -0.25 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -1.731 0.25 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -1.731 0.750001 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at -1.731 1.25 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at -1.731 1.749999 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at -1.731 2.250001 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at -0.750001 2.695999) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at 0.750001 2.695999) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at 1.731 2.250001 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at 1.731 1.749999 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at 1.731 1.25 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd rect (at 1.731 0.750001 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd rect (at 1.731 0.25 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd rect (at 1.731 -0.25 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd rect (at 1.731 -0.750001 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 21 smd rect (at 1.731 -1.25 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 22 smd rect (at 1.731 -1.749999 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 23 smd rect (at 1.731 -2.250001 90) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 24 smd rect (at 0.750001 -2.695999) (size 0.28 0.85) (layers F.Cu F.Paste F.Mask))
  (pad 25 smd rect (at 0 0) (size 2.05 3.099999) (layers F.Cu F.Paste F.Mask))
  (pad V thru_hole circle (at -0.3937 0.7874) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask))
  (pad V thru_hole circle (at -0.3937 0) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask))
  (pad V thru_hole circle (at -0.3937 -0.7874) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask))
  (pad V thru_hole circle (at 0.3937 0.7874) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask))
  (pad V thru_hole circle (at 0.3937 0) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask))
  (pad V thru_hole circle (at 0.3937 -0.7874) (size 0.508 0.508) (drill 0.254) (layers *.Cu *.Mask))
)
