(module BQ40Z50RSMR-R2 (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value RSM32_1P5X1P5_TEX (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.016in/0.4mm" (at -5.9309 0) (layer Cmts.User))
  (fp_text user "0.155in/3.937mm" (at 0 7.6708) (layer Cmts.User))
  (fp_text user "0.155in/3.937mm" (at 9.9822 0) (layer Cmts.User))
  (fp_text user "0.032in/0.813mm" (at 1.9685 -5.0165) (layer Cmts.User))
  (fp_text user "0.009in/0.229mm" (at -7.6708 -1.4) (layer Cmts.User))
  (fp_text user "0.059in/1.5mm" (at 0 5.1308) (layer Cmts.User))
  (fp_text user "0.059in/1.5mm" (at 4.9022 0) (layer Cmts.User))
  (fp_text user "*" (at 1.4 -3.1115) (layer F.SilkS))
  (fp_text user "*" (at 1.4 -1.8161) (layer F.Fab))
  (pad 1 smd rect (at 1.4 -1.9685) (size 0.2286 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 1.000001 -1.9685) (size 0.2286 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 0.599999 -1.9685) (size 0.2286 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 0.2 -1.9685) (size 0.2286 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -0.2 -1.9685) (size 0.2286 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -0.599999 -1.9685) (size 0.2286 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -1.000001 -1.9685) (size 0.2286 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -1.4 -1.9685) (size 0.2286 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at -1.9685 -1.4 90) (size 0.2286 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at -1.9685 -1.000001 90) (size 0.2286 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at -1.9685 -0.599999 90) (size 0.2286 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at -1.9685 -0.2 90) (size 0.2286 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at -1.9685 0.2 90) (size 0.2286 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at -1.9685 0.599999 90) (size 0.2286 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at -1.9685 1.000001 90) (size 0.2286 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at -1.9685 1.4 90) (size 0.2286 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd rect (at -1.4 1.9685) (size 0.2286 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd rect (at -1.000001 1.9685) (size 0.2286 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd rect (at -0.599999 1.9685) (size 0.2286 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd rect (at -0.2 1.9685) (size 0.2286 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 21 smd rect (at 0.2 1.9685) (size 0.2286 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 22 smd rect (at 0.599999 1.9685) (size 0.2286 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 23 smd rect (at 1.000001 1.9685) (size 0.2286 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 24 smd rect (at 1.4 1.9685) (size 0.2286 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 25 smd rect (at 1.9685 1.4 90) (size 0.2286 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 26 smd rect (at 1.9685 1.000001 90) (size 0.2286 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 27 smd rect (at 1.9685 0.599999 90) (size 0.2286 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 28 smd rect (at 1.9685 0.2 90) (size 0.2286 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 29 smd rect (at 1.9685 -0.2 90) (size 0.2286 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 30 smd rect (at 1.9685 -0.599999 90) (size 0.2286 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 31 smd rect (at 1.9685 -1.000001 90) (size 0.2286 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad 32 smd rect (at 1.9685 -1.4 90) (size 0.2286 0.8128) (layers F.Cu F.Paste F.Mask))
  (pad HTAB smd rect (at 0 0) (size 1.5 1.5) (layers F.Cu F.Paste F.Mask))
  (pad V thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.889) (layers *.Cu *.Mask))
)
