(footprint "BUZZER_MAS800_MAL" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tags "MAS800Q ")
  (attr through_hole)
  (fp_text reference "REF**" (at 7.5 0 unlocked) (layer F.SilkS))
  (fp_text value BUZZER_MAS800_MAL (at 7.5 0 unlocked) (layer F.Fab))
  (fp_text user "${REFERENCE}" (at 7.5 0 unlocked) (layer F.Fab))
  (pad "1" thru_hole rect (at 0 0) (size 1.5748 1.5748) (drill 1.0668) (layers *.Cu *.Mask))
  (pad "2" thru_hole circle (at 15.000001 0) (size 1.5748 1.5748) (drill 1.0668) (layers *.Cu *.Mask))
)
