(module Connector_BarrelJack:BarrelJack_CUI_PJ-063AH_Horizontal (layer F.Cu) (tedit 62965FA3)
  (descr "Barrel Jack, 2.0mm ID, 5.5mm OD, 24V, 8A, no switch, https://www.cui.com/product/resource/pj-063ah.pdf")
  (tags "barrel jack cui dc power")
  (fp_text reference REF** (at 0 -2.3) (layer F.SilkS))
  (fp_text value BarrelJack_CUI_PJ-063AH_Horizontal (at 0 13) (layer F.Fab))
  (pad "" thru_hole circle (at 0 9) (size 1.6 1.6) (drill 1.6) (layers *.Cu *.Mask))
  (pad MP2 thru_hole oval (at 4.5 7) (size 2 3.5) (drill oval 1 2.5) (layers *.Cu *.Mask))
  (pad MP1 thru_hole oval (at -4.5 7) (size 2 3.5) (drill oval 1 2.5) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 0 6) (size 3.3 2) (drill oval 2.3 1) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 0 0) (size 4 2) (drill oval 3 1) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Connector_BarrelJack.3dshapes/BarrelJack_CUI_PJ-063AH_Horizontal.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
