(module Bosch_LGA-8_3x3mm_P0.8mm_ClockwisePinNumbering (layer F.Cu) (tedit 5D9F7937)
  (descr "Bosch  LGA, 8 Pin (https://ae-bst.resource.bosch.com/media/_tech/media/datasheets/BST-BME680-DS001-00.pdf#page=44), generated with kicad-footprint-generator ipc_noLead_generator.py")
  (tags "Bosch LGA NoLead")
  (attr smd)
  (fp_text reference REF** (at 0 -2.45) (layer F.SilkS))
  (fp_text value Bosch_LGA-8_3x3mm_P0.8mm_ClockwisePinNumbering (at 0 2.45) (layer F.Fab))
  (pad 1 smd rect (at -1.2 -1.1875) (size 0.5 0.525) (layers F.Cu F.Mask F.Paste))
  (pad 2 smd rect (at -0.4 -1.1875) (size 0.5 0.525) (layers F.Cu F.Mask F.Paste))
  (pad 3 smd rect (at 0.4 -1.1875) (size 0.5 0.525) (layers F.Cu F.Mask F.Paste))
  (pad 4 smd rect (at 1.2 -1.1875) (size 0.5 0.525) (layers F.Cu F.Mask F.Paste))
  (pad 5 smd rect (at 1.2 1.1875) (size 0.5 0.525) (layers F.Cu F.Mask F.Paste))
  (pad 6 smd rect (at 0.4 1.1875) (size 0.5 0.525) (layers F.Cu F.Mask F.Paste))
  (pad 7 smd rect (at -0.4 1.1875) (size 0.5 0.525) (layers F.Cu F.Mask F.Paste))
  (pad 8 smd rect (at -1.2 1.1875) (size 0.5 0.525) (layers F.Cu F.Mask F.Paste))
  (fp_text user %R (at 0 0) (layer F.Fab))
  (model ${KISYS3DMOD}/Package_LGA.3dshapes/Bosch_LGA-8_3x3mm_P0.8mm_ClockwisePinNumbering.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)