(footprint "CAP_PXG_F61_NIP" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tags "APXG160ARA181MF61G ")
  (attr smd)
  (fp_text reference "REF**" (at 0 0 unlocked) (layer F.SilkS))
  (fp_text value CAP_PXG_F61_NIP (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer F.Fab))
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -1.0033 -0.6604)
        (xy 1.0033 -0.6604)
        (xy 1.0033 0.6604)
        (xy -1.0033 0.6604)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -3.3528 -3.3528)
        (xy 3.3528 -3.3528)
        (xy 3.3528 -0.6604)
        (xy -3.3528 -0.6604)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -3.3528 0.6604)
        (xy 3.3528 0.6604)
        (xy 3.3528 3.3528)
        (xy -3.3528 3.3528)
      )
    )
  )
  (pad "1" smd rect (at -2.6289 0) (size 3.1496 1.2192) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at 2.6289 0) (size 3.1496 1.2192) (layers "F.Cu" "F.Paste" "F.Mask"))
)
