(footprint "CAP_YX_12P5X20_RUB" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tags "50ZLJ560M12.5X20 ")
  (attr through_hole)
  (fp_text reference "REF**" (at 2.5 0 unlocked) (layer F.SilkS))
  (fp_text value CAP_YX_12P5X20_RUB (at 2.5 0 unlocked) (layer F.Fab))
  (fp_text user "${REFERENCE}" (at 2.5 0 unlocked) (layer F.Fab))
  (pad "1" thru_hole circle (at 0 0) (size 1.3716 1.3716) (drill 0.8636) (layers *.Cu *.Mask))
  (pad "2" thru_hole circle (at 5 0) (size 1.3716 1.3716) (drill 0.8636) (layers *.Cu *.Mask))
)
