(module CD4051BE (layer F.Cu)
  (fp_text reference REF** (at -3.81 -8.89) (layer F.SilkS))
  (fp_text value N16 (at -3.81 -8.89) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user ".1in/2.54mm" (at -10.668 -16.51) (layer Cmts.User))
  (fp_text user ".051in/1.295mm" (at 3.048 -17.78) (layer Cmts.User))
  (fp_text user ".3in/7.62mm" (at -3.81 -21.1455) (layer Cmts.User))
  (fp_text user ".051in/1.295mm" (at -7.62 3.3655) (layer Cmts.User))
  (fp_text user "*" (at -7.62 -19.1897) (layer F.Fab))
  (fp_text user "*" (at -7.62 -19.1897) (layer F.SilkS))
  (pad 1 thru_hole rect (at -7.62 -17.78) (size 1.2954 1.2954) (drill 0.7874) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -7.62 -15.24) (size 1.2954 1.2954) (drill 0.7874) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at -7.62 -12.7) (size 1.2954 1.2954) (drill 0.7874) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at -7.62 -10.16) (size 1.2954 1.2954) (drill 0.7874) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at -7.62 -7.62) (size 1.2954 1.2954) (drill 0.7874) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at -7.62 -5.08) (size 1.2954 1.2954) (drill 0.7874) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at -7.62 -2.54) (size 1.2954 1.2954) (drill 0.7874) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at -7.62 0) (size 1.2954 1.2954) (drill 0.7874) (layers *.Cu *.Mask))
  (pad 9 thru_hole circle (at 0 0) (size 1.2954 1.2954) (drill 0.7874) (layers *.Cu *.Mask))
  (pad 10 thru_hole circle (at 0 -2.54) (size 1.2954 1.2954) (drill 0.7874) (layers *.Cu *.Mask))
  (pad 11 thru_hole circle (at 0 -5.08) (size 1.2954 1.2954) (drill 0.7874) (layers *.Cu *.Mask))
  (pad 12 thru_hole circle (at 0 -7.62) (size 1.2954 1.2954) (drill 0.7874) (layers *.Cu *.Mask))
  (pad 13 thru_hole circle (at 0 -10.16) (size 1.2954 1.2954) (drill 0.7874) (layers *.Cu *.Mask))
  (pad 14 thru_hole circle (at 0 -12.7) (size 1.2954 1.2954) (drill 0.7874) (layers *.Cu *.Mask))
  (pad 15 thru_hole circle (at 0 -15.24) (size 1.2954 1.2954) (drill 0.7874) (layers *.Cu *.Mask))
  (pad 16 thru_hole circle (at 0 -17.78) (size 1.2954 1.2954) (drill 0.7874) (layers *.Cu *.Mask))
)
