(footprint "CH32V003F4P6" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (attr smd)
  (fp_text reference "REF**" (at -12.7 -7.62 unlocked) (layer "F.SilkS"))
  (fp_text value "CH32V003F4P6" (at 0 15.24 unlocked) (layer "F.Fab"))
  (fp_text user "${REFERENCE}" (at -12.7 15.24 unlocked) (layer "F.Fab"))
  (pad "1" smd rect (at -2.925 2.7) (size 0.25 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "2" smd rect (at -2.275 2.7) (size 0.25 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "3" smd rect (at -1.625 2.7) (size 0.25 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "4" smd rect (at -0.975 2.7) (size 0.25 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "5" smd rect (at -0.325 2.7) (size 0.25 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "6" smd rect (at 0.325 2.7) (size 0.25 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "7" smd rect (at 0.975 2.7) (size 0.25 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "8" smd rect (at 1.625 2.7) (size 0.25 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "9" smd rect (at 2.275 2.7) (size 0.25 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "10" smd rect (at 2.925 2.7) (size 0.25 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "11" smd rect (at 2.925 -2.7) (size 0.25 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "12" smd rect (at 2.275 -2.7) (size 0.25 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "13" smd rect (at 1.625 -2.7) (size 0.25 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "14" smd rect (at 0.975 -2.7) (size 0.25 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "15" smd rect (at 0.325 -2.7) (size 0.25 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "16" smd rect (at -0.325 -2.7) (size 0.25 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "17" smd rect (at -0.975 -2.7) (size 0.25 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "18" smd rect (at -1.625 -2.7) (size 0.25 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "19" smd rect (at -2.275 -2.7) (size 0.25 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
  (pad "20" smd rect (at -2.925 -2.7) (size 0.25 1) (layers "F.Cu" "F.Paste" "F.Mask")
    (thermal_bridge_angle 45))
)
