(footprint "CONN4_3920000_WED" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tags "9993920000 ")
  (attr through_hole)
  (fp_text reference "REF**" (at 7.62 0 unlocked) (layer F.SilkS))
  (fp_text value CONN4_3920000_WED (at 7.62 0 unlocked) (layer F.Fab))
  (fp_text user "${REFERENCE}" (at 7.62 0 unlocked) (layer F.Fab))
  (pad "1" thru_hole circle (at 0 0) (size 1.905 1.905) (drill 1.397) (layers *.Cu *.Mask))
  (pad "2" thru_hole circle (at 5.08 0) (size 1.905 1.905) (drill 1.397) (layers *.Cu *.Mask))
  (pad "3" thru_hole circle (at 10.16 0) (size 1.905 1.905) (drill 1.397) (layers *.Cu *.Mask))
  (pad "4" thru_hole circle (at 15.24 0) (size 1.905 1.905) (drill 1.397) (layers *.Cu *.Mask))
)
