(footprint "CONN5_WR-TBL-1377_WRE" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tags "691137710005 ")
  (attr through_hole)
  (fp_text reference "REF**" (at 10 0 unlocked) (layer F.SilkS))
  (fp_text value CONN5_WR-TBL-1377_WRE (at 10 0 unlocked) (layer F.Fab))
  (fp_text user "${REFERENCE}" (at 10 0 unlocked) (layer F.Fab))
  (pad "1" thru_hole circle (at 0 0) (size 1.8034 1.8034) (drill 1.2954) (layers *.Cu *.Mask))
  (pad "2" thru_hole circle (at 5 0) (size 1.8034 1.8034) (drill 1.2954) (layers *.Cu *.Mask))
  (pad "3" thru_hole circle (at 10 0) (size 1.8034 1.8034) (drill 1.2954) (layers *.Cu *.Mask))
  (pad "4" thru_hole circle (at 15.000001 0) (size 1.8034 1.8034) (drill 1.2954) (layers *.Cu *.Mask))
  (pad "5" thru_hole circle (at 20.000001 0) (size 1.8034 1.8034) (drill 1.2954) (layers *.Cu *.Mask))
)
