(footprint "CONN6x1_BM06B-SURS-TF_JST" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tags "BM06B-SURS-TF ")
  (attr smd)
  (fp_text reference "REF**" (at 0 -0.947674 unlocked) (layer F.SilkS))
  (fp_text value CONN6x1_BM06B-SURS-TF_JST (at 0 -0.947674 unlocked) (layer F.Fab))
  (fp_text user "${REFERENCE}" (at 0 -0.947674 unlocked) (layer F.Fab))
  (pad "1" smd rect (at -2.000001 -0.947674) (size 0.508 1.0922) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at -1.2 -0.947674) (size 0.508 1.0922) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at -0.399999 -0.947674) (size 0.508 1.0922) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd rect (at 0.399999 -0.947674) (size 0.508 1.0922) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "5" smd rect (at 1.2 -0.947674) (size 0.508 1.0922) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "6" smd rect (at 1.999999 -0.947674) (size 0.508 1.0922) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "7" smd rect (at -3.299998 0.452326) (size 1.1938 1.7018) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "8" smd rect (at 3.299998 0.452326) (size 1.1938 1.7018) (layers "F.Cu" "F.Paste" "F.Mask"))
)
