(footprint "CONN_43814-6621_MOL" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tags "438146621 ")
  (attr through_hole)
  (fp_text reference "REF**" (at 8.58 0 unlocked) (layer F.SilkS))
  (fp_text value CONN_43814-6621_MOL (at 8.58 0 unlocked) (layer F.Fab))
  (fp_text user "${REFERENCE}" (at 8.58 0 unlocked) (layer F.Fab))
  (pad "1" thru_hole circle (at 0 0) (size 1.397 1.397) (drill 0.889) (layers *.Cu *.Mask))
  (pad "2" thru_hole circle (at 1.02 -2.030001) (size 1.397 1.397) (drill 0.889) (layers *.Cu *.Mask))
  (pad "3" thru_hole circle (at 2.040001 0) (size 1.397 1.397) (drill 0.889) (layers *.Cu *.Mask))
  (pad "4" thru_hole circle (at 3.059999 -2.030001) (size 1.397 1.397) (drill 0.889) (layers *.Cu *.Mask))
  (pad "5" thru_hole circle (at 4.079999 0) (size 1.397 1.397) (drill 0.889) (layers *.Cu *.Mask))
  (pad "6" thru_hole circle (at 5.1 -2.030001) (size 1.397 1.397) (drill 0.889) (layers *.Cu *.Mask))
  (pad "12" thru_hole circle (at 17.160001 -2.030001) (size 1.397 1.397) (drill 0.889) (layers *.Cu *.Mask))
  (pad "11" thru_hole circle (at 16.14 0) (size 1.397 1.397) (drill 0.889) (layers *.Cu *.Mask))
  (pad "10" thru_hole circle (at 15.12 -2.030001) (size 1.397 1.397) (drill 0.889) (layers *.Cu *.Mask))
  (pad "9" thru_hole circle (at 14.100002 0) (size 1.397 1.397) (drill 0.889) (layers *.Cu *.Mask))
  (pad "8" thru_hole circle (at 13.080001 -2.030001) (size 1.397 1.397) (drill 0.889) (layers *.Cu *.Mask))
  (pad "7" thru_hole circle (at 12.060001 0) (size 1.397 1.397) (drill 0.889) (layers *.Cu *.Mask))
  (pad "13" np_thru_hole circle (at -2.215 3.049999) (size 3.302 3.302) (drill 3.302) (layers))
  (pad "14" np_thru_hole circle (at 19.375 3.049999) (size 3.302 3.302) (drill 3.302) (layers))
)
