(footprint CONV_REM2A-0505S (layer F.Cu) (tedit 67B4B6C4)
  (descr "")
  (fp_text reference REF** (at -9.325 -8.425 0) (layer F.SilkS))
  (fp_text value CONV_REM2A-0505S (at -2.34 8.365 0) (layer F.Fab))
  (pad 1 thru_hole rect (at -8.89 5.08) (size 1.408 1.408) (drill 0.9) (layers *.Cu *.Mask) (solder_mask_margin 0.102))
  (pad 2 thru_hole circle (at -6.35 5.08) (size 1.408 1.408) (drill 0.9) (layers *.Cu *.Mask) (solder_mask_margin 0.102))
  (pad 7 thru_hole circle (at 6.35 5.08) (size 1.408 1.408) (drill 0.9) (layers *.Cu *.Mask) (solder_mask_margin 0.102))
  (pad 8 thru_hole circle (at 8.89 5.08) (size 1.408 1.408) (drill 0.9) (layers *.Cu *.Mask) (solder_mask_margin 0.102))
  (pad 9 thru_hole circle (at 8.89 -5.08) (size 1.408 1.408) (drill 0.9) (layers *.Cu *.Mask) (solder_mask_margin 0.102))
  (pad 10 thru_hole circle (at 6.35 -5.08) (size 1.408 1.408) (drill 0.9) (layers *.Cu *.Mask) (solder_mask_margin 0.102))
  (pad 16 thru_hole circle (at -8.89 -5.08) (size 1.408 1.408) (drill 0.9) (layers *.Cu *.Mask) (solder_mask_margin 0.102))
  (zone (net 0) (net_name "") (layer F.Cu) (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.01)
    (keepout (tracks not_allowed) (vias not_allowed) (pads not_allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -4.0 -7.75)
        (xy 4.0 -7.75)
        (xy 4.0 7.75)
        (xy -4.0 7.75)
      )
    )
  )
  (zone (net 0) (net_name "") (layers *.Cu) (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.01)
    (keepout (tracks allowed) (vias not_allowed) (pads allowed ) (copperpour allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -4.0 -7.75)
        (xy 4.0 -7.75)
        (xy 4.0 7.75)
        (xy -4.0 7.75)
      )
    )
  )
)