(module CPC1014NTR (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value CPC1014N_IXY (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.1in/2.54mm" (at -5.8039 0) (layer Cmts.User))
  (fp_text user "0.017in/0.432mm" (at 5.8039 -1.27) (layer Cmts.User))
  (fp_text user "0.217in/5.512mm" (at 0 -4.4704) (layer Cmts.User))
  (fp_text user "0.055in/1.397mm" (at -2.7559 4.4704) (layer Cmts.User))
  (fp_text user "*" (at -3.0099 -2.8448) (layer F.SilkS))
  (fp_text user "*" (at -1.5367 -1.9812) (layer F.Fab))
  (pad 1 smd rect (at -2.7559 -1.27) (size 1.397 0.4318) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -2.7559 1.27) (size 1.397 0.4318) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 2.7559 1.27) (size 1.397 0.4318) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 2.7559 -1.27) (size 1.397 0.4318) (layers F.Cu F.Paste F.Mask))
)
