(module CP_EIA-3216-18_Kemet-A_Pad1.58x1.35mm_HandSolder (layer F.Cu) (tedit 5EBA9318)
  (descr "Tantalum Capacitor SMD Kemet-A (3216-18 Metric), IPC_7351 nominal, (Body size from: http://www.kemet.com/Lists/ProductCatalog/Attachments/253/KEM_TC101_STD.pdf), generated with kicad-footprint-generator")
  (tags "capacitor tantalum")
  (attr smd)
  (fp_text reference REF** (at 0 -1.75) (layer F.SilkS))
  (fp_text value CP_EIA-3216-18_Kemet-A_Pad1.58x1.35mm_HandSolder (at 0 1.75) (layer F.Fab))
  (pad 1 smd roundrect (at -1.4375 0) (size 1.575 1.35) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.185185))
  (pad 2 smd roundrect (at 1.4375 0) (size 1.575 1.35) (layers F.Cu F.Mask F.Paste) (roundrect_rratio 0.185185))
  (fp_text user %R (at 0 0) (layer F.Fab))
  (model ${KISYS3DMOD}/Capacitor_Tantalum_SMD.3dshapes/CP_EIA-3216-18_Kemet-A.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)