(module CR1206-FX-4701ELF (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value BO_CR1206 (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.069in/1.753mm" (at 4.7752 0) (layer Cmts.User))
  (fp_text user "0.164in/4.166mm" (at 0 -3.9243) (layer Cmts.User))
  (fp_text user "0.076in/1.93mm" (at 0 3.9243) (layer Cmts.User))
  (pad 1 smd rect (at -1.524 0) (size 1.1176 1.7526) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 1.524 0) (size 1.1176 1.7526) (layers F.Cu F.Paste F.Mask))
)
