(module C_Axial_L19.0mm_D9.0mm_P25.00mm_Horizontal (layer F.Cu) (tedit 5AE50EF0)
  (descr "C, Axial series, Axial, Horizontal, pin pitch=25mm, , length*diameter=19*9mm^2, http://cdn-reichelt.de/documents/datenblatt/B300/STYROFLEX.pdf")
  (tags "C Axial series Axial Horizontal pin pitch 25mm  length 19mm diameter 9mm")
  (fp_text reference REF** (at 12.5 -5.62) (layer F.SilkS))
  (fp_text value C_Axial_L19.0mm_D9.0mm_P25.00mm_Horizontal (at 12.5 5.62) (layer F.Fab))
  (pad 1 thru_hole circle (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 25 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask))
  (fp_text user %R (at 12.5 0) (layer F.Fab))
  (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/C_Axial_L19.0mm_D9.0mm_P25.00mm_Horizontal.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)