(module Core4 (layer F.Cu) (tedit 5CAB97C3)
  (fp_text reference REF** (at 23.34 63.42) (layer F.SilkS))
  (fp_text value Core4 (at 23.7 -1.4) (layer F.Fab))
  (pad 25 thru_hole circle (at 46.53 -0.06) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 1 thru_hole circle (at 0 0) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 0 2.54) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 0 5.08) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 0 7.62) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 0 10.16) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 0 12.7) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at 0 15.24) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at 0 17.78) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 9 thru_hole circle (at 0 20.32) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 10 thru_hole circle (at 0 22.86) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 11 thru_hole circle (at 0 25.4) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 12 thru_hole circle (at 0 27.94) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 13 thru_hole circle (at 0 30.48) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 14 thru_hole circle (at 0 33.02) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 15 thru_hole circle (at 0 35.56) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 16 thru_hole circle (at 0 38.1) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 17 thru_hole circle (at 0 40.64) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 18 thru_hole circle (at 0 43.18) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 19 thru_hole circle (at 0 45.72) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 20 thru_hole circle (at 0 48.26) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 21 thru_hole circle (at 0 50.8) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 22 thru_hole circle (at 0 53.34) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 23 thru_hole circle (at 0 55.88) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 24 thru_hole circle (at 0 58.42) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad "" thru_hole circle (at 1 -5) (size 5.5 5.5) (drill 3.5) (layers *.Cu *.Mask))
  (pad "" thru_hole circle (at 1 63.4) (size 5.5 5.5) (drill 3.5) (layers *.Cu *.Mask))
  (pad "" thru_hole circle (at 45.65 63.39) (size 5.5 5.5) (drill 3.5) (layers *.Cu *.Mask))
  (pad "" thru_hole circle (at 45.65 -5.02) (size 5.5 5.5) (drill 3.5) (layers *.Cu *.Mask))
  (pad 49 thru_hole circle (at 23.42 23.75) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 26 thru_hole circle (at 46.53 2.48) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 27 thru_hole circle (at 46.53 5.02) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 28 thru_hole circle (at 46.53 7.56) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 29 thru_hole circle (at 46.53 10.1) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 30 thru_hole circle (at 46.53 12.64) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 31 thru_hole circle (at 46.53 15.18) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 32 thru_hole circle (at 46.53 17.72) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 33 thru_hole circle (at 46.53 20.26) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 34 thru_hole circle (at 46.53 22.8) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 35 thru_hole circle (at 46.53 25.34) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 36 thru_hole circle (at 46.53 27.88) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 37 thru_hole circle (at 46.53 30.42) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 38 thru_hole circle (at 46.53 32.96) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 39 thru_hole circle (at 46.53 35.5) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 40 thru_hole circle (at 46.53 38.04) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 41 thru_hole circle (at 46.53 40.58) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 42 thru_hole circle (at 46.53 43.12) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 43 thru_hole circle (at 46.53 45.66) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 44 thru_hole circle (at 46.53 48.2) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 45 thru_hole circle (at 46.53 50.74) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 46 thru_hole circle (at 46.53 53.28) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 47 thru_hole circle (at 46.53 55.82) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 48 thru_hole circle (at 46.53 58.36) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 50 thru_hole circle (at 23.42 26.29) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 51 thru_hole circle (at 25.96 23.75) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 52 thru_hole circle (at 25.96 26.29) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 53 thru_hole circle (at 28.5 23.75) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 54 thru_hole circle (at 28.5 26.29) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 55 thru_hole circle (at 31.04 23.75) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 56 thru_hole circle (at 31.04 26.29) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 57 thru_hole circle (at 33.58 23.75) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 58 thru_hole circle (at 33.58 26.29) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 59 thru_hole circle (at 36.12 23.75) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 60 thru_hole circle (at 36.12 26.29) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 61 thru_hole circle (at 38.66 23.75) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (pad 62 thru_hole circle (at 38.66 26.29) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask))
  (model "C:/Users/Administrator.DESKTOP-N5DN21F/Desktop/Fiverr/Clients/z Small Scale/`jama_b/footprint/core4.pretty/Core4_Black_PCB.step"
    (offset (xyz 104.6555 -59.65 13))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model "C:/Users/Administrator.DESKTOP-N5DN21F/Desktop/Fiverr/Clients/z Small Scale/`jama_b/footprint/core4.pretty/PinSocket_1x24_P2.54mm_Vertical.step"
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model "C:/Users/Administrator.DESKTOP-N5DN21F/Desktop/Fiverr/Clients/z Small Scale/`jama_b/footprint/core4.pretty/PinSocket_1x24_P2.54mm_Vertical.step"
    (offset (xyz 46.55 0.05 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model ${KIPRJMOD}/core4.pretty/PinSocket_2x07_P2.54mm_Vertical.step
    (offset (xyz 38.6841994190216 -26.28899960517883 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 90))
  )
)
