(module DAC80501ZDGSR (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value DGS10_TEX (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.02in/0.5mm" (at -5.26415 -0.75) (layer Cmts.User))
  (fp_text user "0.011in/0.279mm" (at 5.26415 -1) (layer Cmts.User))
  (fp_text user "0.174in/4.432mm" (at 0 -3.9624) (layer Cmts.User))
  (fp_text user "0.052in/1.334mm" (at -2.21615 3.9624) (layer Cmts.User))
  (fp_text user "*" (at -2.47015 -2.4224) (layer F.SilkS))
  (fp_text user "*" (at -1.1684 -1.4732) (layer F.Fab))
  (pad 1 smd rect (at -2.21615 -1.000001) (size 1.3335 0.2794) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -2.21615 -0.499999) (size 1.3335 0.2794) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -2.21615 0) (size 1.3335 0.2794) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -2.21615 0.499999) (size 1.3335 0.2794) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -2.21615 1.000001) (size 1.3335 0.2794) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 2.21615 1.000001) (size 1.3335 0.2794) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 2.21615 0.499999) (size 1.3335 0.2794) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 2.21615 0) (size 1.3335 0.2794) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 2.21615 -0.499999) (size 1.3335 0.2794) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 2.21615 -1.000001) (size 1.3335 0.2794) (layers F.Cu F.Paste F.Mask))
)
