(footprint "DEF0008A-IPC_A" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tags "HDC3020DEFR ")
  (attr smd)
  (fp_text reference "REF**" (at 0 0 unlocked) (layer F.SilkS))
  (fp_text value DEF0008A-IPC_A (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "Designator98" (at -2.286 -3.0226 unlocked) (layer "F.SilkS"))
  (pad "1" smd rect (at -1.225532 -0.750001) (size 0.961067 0.242473) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at -1.225532 -0.25) (size 0.961067 0.242473) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at -1.225532 0.25) (size 0.961067 0.242473) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd rect (at -1.225532 0.750001) (size 0.961067 0.242473) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "5" smd rect (at 1.225532 0.750001) (size 0.961067 0.242473) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "6" smd rect (at 1.225532 0.25) (size 0.961067 0.242473) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "7" smd rect (at 1.225532 -0.25) (size 0.961067 0.242473) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "8" smd rect (at 1.225532 -0.750001) (size 0.961067 0.242473) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "9" smd rect (at 0 0) (size 1.3 2.000001) (layers "F.Cu" "F.Mask"))
)
