(module DFE322512F-3R3M=P2 (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value IND_DFE322512F_MUR (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.106in/2.692mm" (at 4.7498 0) (layer Cmts.User))
  (fp_text user "0.162in/4.115mm" (at 0 -4.3942) (layer Cmts.User))
  (fp_text user "0.07in/1.778mm" (at 0 4.3942) (layer Cmts.User))
  (pad 1 smd rect (at -1.4732 0) (size 1.1684 2.6924) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 1.4732 0) (size 1.1684 2.6924) (layers F.Cu F.Paste F.Mask))
)
