(footprint "DFN-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "6-Lead Plastic Dual Flat, No Lead Package (MA) - 2x2x0.9 mm Body [DFN] (see Microchip Packaging Specification 00000049BS.pdf)")
	(tags "DFN 0.65")
	(property "Reference" "REF**"
		(at 0 -2.025 0)
		(layer "F.SilkS")
	)
	(property "Value" "DFN-6-1EP_2x2mm_P0.65mm_EP1x1.6mm"
		(at 0 2.025 0)
		(layer "F.Fab")
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at 0 -0.4)
		(size 0.82 0.63)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at 0 0.4)
		(size 0.82 0.63)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -1.05 -0.65)
		(size 0.65 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "2" smd rect
		(at -1.05 0)
		(size 0.65 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "3" smd rect
		(at -1.05 0.65)
		(size 0.65 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "4" smd rect
		(at 1.05 0.65)
		(size 0.65 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "5" smd rect
		(at 1.05 0)
		(size 0.65 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "6" smd rect
		(at 1.05 -0.65)
		(size 0.65 0.35)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "7" smd rect
		(at 0 0)
		(size 1 1.6)
		(layers "F.Cu" "F.Mask")
	)
	(model "${KICAD8_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/DFN-6-1EP_2x2mm_P0.65mm_EP1x1.6mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)