(module DFN-6-1EP_3x2mm_P0.5mm_EP1.65x1.35mm (layer F.Cu) (tedit 5DC5F54E)
  (descr "DFN, 6 Pin (https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/ltc-legacy-dfn/(DCB6)%20DFN%2005-08-1715%20Rev%20A.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
  (tags "DFN NoLead")
  (attr smd)
  (fp_text reference REF** (at 0 -1.95) (layer F.SilkS))
  (fp_text value DFN-6-1EP_3x2mm_P0.5mm_EP1.65x1.35mm (at 0 1.95) (layer F.Fab))
  (pad 1 smd rect (at -1.4375 -0.5) (size 0.825 0.25) (layers F.Cu F.Mask F.Paste))
  (pad 2 smd rect (at -1.4375 0) (size 0.825 0.25) (layers F.Cu F.Mask F.Paste))
  (pad 3 smd rect (at -1.4375 0.5) (size 0.825 0.25) (layers F.Cu F.Mask F.Paste))
  (pad 4 smd rect (at 1.4375 0.5) (size 0.825 0.25) (layers F.Cu F.Mask F.Paste))
  (pad 5 smd rect (at 1.4375 0) (size 0.825 0.25) (layers F.Cu F.Mask F.Paste))
  (pad 6 smd rect (at 1.4375 -0.5) (size 0.825 0.25) (layers F.Cu F.Mask F.Paste))
  (pad 7 smd rect (at 0 0) (size 1.65 1.35) (layers F.Cu F.Mask))
  (pad "" smd rect (at -0.41 -0.34) (size 0.67 0.54) (layers F.Paste))
  (pad "" smd rect (at -0.41 0.34) (size 0.67 0.54) (layers F.Paste))
  (pad "" smd rect (at 0.41 -0.34) (size 0.67 0.54) (layers F.Paste))
  (pad "" smd rect (at 0.41 0.34) (size 0.67 0.54) (layers F.Paste))
  (fp_text user %R (at 0 0) (layer F.Fab))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-6-1EP_3x2mm_P0.5mm_EP1.65x1.35mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)