(module DFN-8-1EP_2x2mm_P0.5mm_EP0.9x1.5mm (layer F.Cu) (tedit 5DC5F54E)
  (descr "DFN, 8 Pin (http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8127-AVR-8-bit-Microcontroller-ATtiny4-ATtiny5-ATtiny9-ATtiny10_Datasheet.pdf), generated with kicad-footprint-generator ipc_noLead_generator.py")
  (tags "DFN NoLead")
  (attr smd)
  (fp_text reference REF** (at 0 -1.95) (layer F.SilkS))
  (fp_text value DFN-8-1EP_2x2mm_P0.5mm_EP0.9x1.5mm (at 0 1.95) (layer F.Fab))
  (pad 1 smd rect (at -1 -0.75) (size 0.7 0.25) (layers F.Cu F.Mask F.Paste))
  (pad 2 smd rect (at -1 -0.25) (size 0.7 0.25) (layers F.Cu F.Mask F.Paste))
  (pad 3 smd rect (at -1 0.25) (size 0.7 0.25) (layers F.Cu F.Mask F.Paste))
  (pad 4 smd rect (at -1 0.75) (size 0.7 0.25) (layers F.Cu F.Mask F.Paste))
  (pad 5 smd rect (at 1 0.75) (size 0.7 0.25) (layers F.Cu F.Mask F.Paste))
  (pad 6 smd rect (at 1 0.25) (size 0.7 0.25) (layers F.Cu F.Mask F.Paste))
  (pad 7 smd rect (at 1 -0.25) (size 0.7 0.25) (layers F.Cu F.Mask F.Paste))
  (pad 8 smd rect (at 1 -0.75) (size 0.7 0.25) (layers F.Cu F.Mask F.Paste))
  (pad 9 smd rect (at 0 0) (size 0.9 1.5) (layers F.Cu F.Mask))
  (pad "" smd rect (at -0.225 -0.375) (size 0.36 0.6) (layers F.Paste))
  (pad "" smd rect (at -0.225 0.375) (size 0.36 0.6) (layers F.Paste))
  (pad "" smd rect (at 0.225 -0.375) (size 0.36 0.6) (layers F.Paste))
  (pad "" smd rect (at 0.225 0.375) (size 0.36 0.6) (layers F.Paste))
  (fp_text user %R (at 0 0) (layer F.Fab))
  (model ${KISYS3DMOD}/Package_DFN_QFN.3dshapes/DFN-8-1EP_2x2mm_P0.5mm_EP0.9x1.5mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)