(footprint "DIP-4_W7.62mm-new" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "4-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
  (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
  (attr through_hole)
  (fp_text reference "REF**" (at 3.81 -2.33) (layer "F.SilkS"))
  (fp_text value "DIP-4_W7.62mm-new" (at 3.81 4.87) (layer "F.Fab"))
  (fp_text user "${REFERENCE}" (at 3.81 1.27) (layer "F.Fab"))
  (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask"))
  (pad "2" thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask"))
  (pad "3" thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask"))
  (pad "4" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask"))
  (model "${KISYS3DMOD}/Package_DIP.3dshapes/DIP-4_W7.62mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
