(module DLF162500LT-5028A1 (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value DLF-4_1P6X0P8 (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0in/0mm" (at -3.8735 0) (layer Cmts.User))
  (fp_text user "0.048in/1.219mm" (at 0 5.9563) (layer Cmts.User))
  (fp_text user "0.018in/0.457mm" (at 8.5979 0) (layer Cmts.User))
  (fp_text user "0.011in/0.279mm" (at 0.2286 -3.6576) (layer Cmts.User))
  (fp_text user "0.028in/0.711mm" (at -6.3373 0) (layer Cmts.User))
  (pad 1 smd rect (at -0.6096 0) (size 0.2794 0.7112) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 0 0.2286 90) (size 0.254 0.4572) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 0.6096 0) (size 0.2794 0.7112) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 0 -0.2286 90) (size 0.254 0.4572) (layers F.Cu F.Paste F.Mask))
)
