(footprint "DMB0006A" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tags "HDC2080DMBR ")
  (attr smd)
  (fp_text reference "REF**" (at 0 0 unlocked) (layer F.SilkS))
  (fp_text value DMB0006A (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer F.Fab))
  (pad "1" smd rect (at -1.4 -1.000001) (size 0.599999 0.399999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at -1.4 0) (size 0.599999 0.399999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at -1.4 1.000001) (size 0.599999 0.399999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd rect (at 1.4 1.000001) (size 0.599999 0.399999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "5" smd rect (at 1.4 0) (size 0.599999 0.399999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "6" smd rect (at 1.4 -1.000001) (size 0.599999 0.399999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "7" smd rect (at 0 0) (size 1.5 2.4) (layers "F.Cu" "F.Mask"))
  (pad "V" thru_hole circle (at -0.499999 0) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "V" thru_hole circle (at 0.499999 0) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "V" thru_hole circle (at 0 -0.950001) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask))
  (pad "V" thru_hole circle (at 0 0.950001) (size 0.499999 0.499999) (drill 0.2032) (layers *.Cu *.Mask))
)
