(module DMC3071LVT-7 (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value TSOT26_DIO (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.037in/0.95mm" (at -4.34975 -0.475) (layer Cmts.User))
  (fp_text user "0.02in/0.508mm" (at 4.34975 -0.95) (layer Cmts.User))
  (fp_text user "0.102in/2.604mm" (at 0 -3.9116) (layer Cmts.User))
  (fp_text user "0.036in/0.902mm" (at -1.30175 3.9116) (layer Cmts.User))
  (fp_text user "*" (at -1.55575 -2.601) (layer F.SilkS))
  (fp_text user "*" (at -0.4699 -1.4224) (layer F.Fab))
  (pad 1 smd rect (at -1.30175 -0.950001) (size 0.9017 0.508) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.30175 0) (size 0.9017 0.508) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.30175 0.950001) (size 0.9017 0.508) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 1.30175 0.950001) (size 0.9017 0.508) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 1.30175 0) (size 0.9017 0.508) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 1.30175 -0.950001) (size 0.9017 0.508) (layers F.Cu F.Paste F.Mask))
)
