(module DSC1001BI2-005.5296 (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value CDFN4_5X3P2_MCH (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.1in/2.54mm" (at -4.200401 0) (layer Cmts.User))
  (fp_text user "0.033in/0.849mm" (at 4.200401 -1.27) (layer Cmts.User))
  (fp_text user "0.091in/2.305mm" (at 0 -4.913) (layer Cmts.User))
  (fp_text user "0.059in/1.505mm" (at -1.152401 4.278) (layer Cmts.User))
  (pad 1 smd rect (at -1.152401 -1.27) (size 1.5048 0.8492) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.152401 1.27) (size 1.5048 0.8492) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 1.152401 1.27) (size 1.5048 0.8492) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 1.152401 -1.27) (size 1.5048 0.8492) (layers F.Cu F.Paste F.Mask))
)
